
**SAFETY COMPLIANCE HECKLIST**



Machine Guarding (continued)

|  |  |  |
| --- | --- | --- |
| **Housekeeping** |  |  |
|  | Is machinery and equipment kept clean and properly maintained? |  |
|  | Is clothing, jewelry, and hair worn by the employee appropriate for machine hazards? |  |
| **Fire Protection** |  |  |
|  | Are all fire extinguishers inspected and recharged regularly, and noted on the inspection tag? | .157 |
|  | Are electrical equipment parts which normally produce arcs, sparks, flames, or molten metal enclosed and separated from all combustible materials? | .303(d) |
|  | Are circuit breakers marked and accessible to personnel, protected from physical damage, and located away from ignitable material? | .304(e)(1)(iv) |
| **Markings** |  |  |
|  | Are manually operated valves and switches controlling the operation of equipment and chines clearly identified and readily accessible? |  |
|  | Are all emergency stop buttons colored red? |  |
| **Lockout Procedures** |  |  |
|  | Can electric power or other energy sources to each machine be locked for maintenance, repair, or security? |  |
|  | Are foot-operated switches guarded or arranged to prevent accidental actuation by personnel or falling objects? |  |
|  | Are revolving drums, barrels, points-of-contact, and containers required to be guarded by an enclosure that is interlocked with the drive mechanism, so that revolution cannot occur unless the guard enclosure is in place? |  |
|  | Are provisions made to prevent machines from automatically starting, or recycling, when power is restored after a power failure or shutdown? |  |

2