STOCK MOWERS

1. CAN USE A TWO (2) INCH PIPE OR SQ TUBING FOR LEG PROTECTORS DOWN BOTH SIDES WELDED TO THE FRAME. CAN BE CONNECTED BEHIND THE SEAT IF YOU CHOOSE TO DO SO.
2. CAN USE 2X2 ANGLE DOWN BOTH SIDES OF THE FRAME TO HOOK LEG PROTECTORS TO.
3. BATTERY MUST BE REMOVED.
4. GAS TANK MUST BE STRAPPED AND SECURED.
5. NO OTHER METAL IS TO BE ADDED TO THE FRAME OR WELDING OF THE FRAME IS ALLOWED OTHER THEN WHAT IS STATED IN THE RULES.
6. IF MOWER QUITS, YOU’RE OUT! IF YOU ROLL YOUR MOWER OVER, YOU’RE OUT! IF YOUR MOWER CATCHES FIRE, YOU’RE OUT!
7. IF USING SOLID SHEETING ON LEG PROTECTORS AND BACK PROTECTOR. METAL CANNOT BE ANY THICKER THEN 1/8 INCH. SEAT PROTECTOR CANNOT BE MORE THEN 6 INCHES ABOVE THE SEAT.
8. 14 HP or less motor.
9. Factory pullys MUST BE STOCK!
10. Factory body’s
11. Governors must be hooked up. No overriding governor.