|  |  |
| --- | --- |
| **GEN-1320** (120V-2500W-15.8kW-60Hz) | **Geneforce Emergency Power System** |
| **Product Features** |
| Silent operation. |
| Safe for indoors. No gas or emissions. |
| No Installation; No Maintenance; No Permits required |
| Arrives fully charged and ready to work. |
| Automatic & one-touch start. |
| Multi-colored LED displays state of charge, AC input, DC volts and DC amperage, etc... |
| Overheat Temperature Sensor & Automatic Shutdown feature. |
| Built-in voltage regulation system for sensitive electronics. |
| Built-in (120V/30A) Automatic A/C Transfer Switch. |
| Built-in 30A solar charge controller for solar panel charging. |
| **Electrical Specifications** | **GEN-1320 (120V)** |
| Output power (continuous) | 2,500 W |
| Surge power (AC amps) | 7,500 W (62.5A) |
| Output frequency regulation | 60 Hz |
| Voltage regulation | 120 V +/-5% true RMS |
| Output wave form | Modified Sine Wave |
| Service Life (No Maintenance) | 12-16 years |
| Energy Stored Inside | 15.8 kW (15,840 Watts) |
| AC output receptacles | Four 20A/120V outlets & One 30A/120V outlet |
| 12 Volt Power Outlet (optional - not included) | One 12 Volt Charger outlet |
| AC input plug (8ft cord) | One (120V/20A) side blade plug \*(30A/120V)optional |
| AC input automatic transfer switch | 30 A (included) |
| Charge rate | 130 A DC |
| AC input voltage range | 90 - 130 VAC |
| Geneforce Charge control | 3-stage (Bulk, Acceptance, Float) |
| Solar Charge Controller | 30A/12V (~360 W per hour/sunlight) \*(60A/12V-24V) optional |
| **General Specifications** |  |
| Optimal operating temperature range | 32°F – 104°F (0°C – 40°C) \*derated below 0°C and above 40°C |
| Monitor | LED Display (reads V, DC amps, Power Share, etc.) |
| Dimensions (H x W x L) and Weight | (36" x 18 x 36") & (1,075 Lbs.) |
| Construction | Strong Steel, Four Casters, Color-Black |
| Warranty & Part Number | 2yr. warranty-components; 4yr. warranty-cells  (GEN-1320-120-2500) |
| **Regulatory Approvals & Protection** |  |
| Safety - UL Listing | Components UL & cUL listed to 458 Standards |
| Voltage Regulation | Over voltage and under voltage protection |
| Temperature | Over-temperature protection |
| Output | Overload Protection |
| Electrical | Short circuit protection |
| **Price** | **$9,997** |
| **Geneforce Incorporated** [**www.geneforcepower.com**](http://www.geneforcepower.com) **(305)215-5443 email:** [**sales@geneforcepower.com**](mailto:sales@geneforcepower.com) | |