**Unity Area Regional Recycling Center**

95 Leonard Rd Phone: (207)568-3117

Thorndike, ME 04986 Fax: (207)568-3319

E-mail: uarrc@uninets.net www.uarrc.org

**GROUND LADDER INSPECTION**

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* All ground ladders must be inspected annually or after exposure to heat, suspected of being unsafe, after being overloaded or after impact or unusual contact.
* All ground ladders must be used, inspected and maintained in accordance with the manufacturer’s guidelines.

\* **Manufacturer’s Name**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \* **Mfg. SERIAL #**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\* **FD # or Apparatus #:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \* **Length:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\* **Ladder Type**: Single ( ) Roof ( ) Extension ( )

Folding( ) Combination ( ) Other ( ) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\* **Construction**: Metal ( ) Wood ( ) Fiberglass ( )

\***Inspect**:

**Beams** (burrs, sharp edges, cracks, splinters, breaks, gouges, checks, wavy conditions) Pass ( ) Fail ( )

**Dogs/Pawl/Locks** (cracks, operation, loose, damaged, lubricated) Pass ( ) Fail ( ) N/A ( )

**Rungs** (snug/tight, bends, burrs, break, welds) Pass ( ) Fail ( )

**Pulley** (damaged, cracks, operational, oiled) Pass ( ) Fail ( ) N/A ( )

**Halyard/Cable** (frayed rope, damaged cable/wire, knots, kinks) Pass ( ) Fail ( ) N/A ( )

**Roof Hooks** (sharp, operational, deformed) Pass ( ) Fail ( ) N/A ( )

**Bolts/rivets** ( tight ) Pass ( ) Fail ( )

**Feet/ Butt spurs** (loose, wear, damaged, operational) Pass ( ) Fail ( )

**Welds** (cracks, broken) Pass ( ) Fail ( )

**Clean Condition** Pass ( ) Fail ( )

**Waxed/Oiled** (extension ladders) Yes ( ) No ( )

**Other**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Pass ( ) Fail ( )

\***Wood ladders** (cracks, splits, not painted except top/bottom 18” for visibility,) Pass ( ) Fail ( ) N/A ( )

**Inspected by**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\* **Damages**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\* All damaged ladders must be removed from service and tagged :

**“OUT OF SERVICE-DO NOT USE”**

\* **Repaired by**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_