|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
|  |
| **http://www.evergreen-marine.com/tuf1/images/item1.gif** | **Dry Cargo Container** |
|  |

|  |  |
| --- | --- |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' Steel Dry Cargo Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 20sd |
| Length | Width | Height |
| 20'-0" | 8'-0" | 8'-6" |
| 6.058 m | 2.438 m | 2.591 m |
| **Interior** |
| Length | Width | Height |
| 19'-4 13/16" | 7'-8 19/32" | 7'-9 57/64" |
| 5.898 m | 2.352 m | 2.385 m |
| **Weight** | **Door Opening** |
| MGW | TARE | NET | Width | Height |
| 52,910 lb | 5,140 lb | 47,770 lb | 7'-8 1/8" | 7'-5 3/4" |
| 67,200 lb | 5,290 lb | 61,910 lb | 2.343 m | 2.280 m |
| 24,000 kg | 2,330 kg | 21,670 kg | **CU.M** | **CU.FT** |
| 30,480 kg | 2,400 kg | 28,080 kg | 33.1 | 1,169 |
| **Purpose** |
| 1.Captioned units(MGW 30,480 KG) can be coordinated from EMCU 3204073 and EISU 3568118.2.Used for all kinds of general cargo.  |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Steel Dry Cargo Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 40sd |
| Length | Width | Height |
| 40'-0" | 8'-0" | 8'-6" |
| 12.192 m | 2.438 m | 2.591 m |
| **Interior** |
| Length | Width | Height |
| 39'-5 45/64" | 7'-8 19/32" | 7'-9 57/64" |
| 12.032 m | 2.352 m | 2.385 m |
| **Weight** | **Door Opening** |
| MGW | TARE | NET | Width | Height |
| 67,200 lb | 8,820 lb | 58,380 lb | 7'-8 1/8" | 7'-5 3/4" |
| 2.343 m | 2.280 m |
| 30,480 kg | 4,000 kg | 26,480 kg | **CU.M** | **CU.FT** |
| 67.5 | 2,385 |
| **Purpose** |
| Used for all kinds of general cargo. |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Hi-Cube Steel Dry Cargo Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 40sh |
| Length | Width | Height |
| 40'-0" | 8'-0" | 9'-6" |
| 12.192 m | 2.438 m | 2.896 m |
| **Interior** |
| Length | Width | Height |
| 39'-5 45/64" | 7'-8 19/32" | 8'-9 15/16" |
| 12.032 m | 2.352 m | 2.69 m |
| **Weight** | **Door Opening** |
| MGW | TARE | NET | Width | Height |
| 67,200 lb | 9,260 lb | 57,940 lb | 7'-8 1/8" | 8'-5 49/64" |
| 2.343 m | 2.585 m |
| 30,480 kg | 4,200 kg | 26,280 kg | **CU.M** | **CU.FT** |
| 76.2 | 2,690 |
| **Purpose** |
| Used for all kinds of general cargo. |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **45' Hi-Cube Steel Dry Cargo Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 45sh |
| Length | Width | Height |
| 45'-0" | 8'-0" | 9'-6" |
| 13.716 m | 2.438 m | 2.896 m |
| **Interior** |
| Length | Width | Height |
| 44'-5 7/10'' | 7'-8 19/32'' | 8'-10 17/64'' |
| 13.556 m | 2.352 m | 2.698 m |
| **Weight** | **Door Opening** |
| MGW | TARE | NET | Width | Height |
| 67,200 lb | 10,580 lb | 56,620 lb | 7'-8 1/8" | 8'-5 3/4" |
| 2.340 m | 2.585 m |
| 30,480 kg | 4,800 kg | 25,680 kg | **CU.M** | **CU.FT** |
| 86.1 | 3,040 |
| **Purpose** |
| Used for all kinds of general cargo. |

|  |  |
| --- | --- |
| **Exterior** | 45sh |
| Length | Width | Height |
| 45'-0" | 8'-0" | 9'-6" |
| 13.716 m | 2.438 m | 2.896 m |
| **Interior** |
| Length | Width | Height |
| 44'-5 7/10'' | 7'-8 19/32'' | 8'-10 17/64'' |
| 13.556 m | 2.352 m | 2.698 m |
| **Weight** | **Door Opening** |
| MGW | TARE | NET | Width | Height |
| 67,200 lb | 10,858 lb | 56,342 lb | 7'-8 1/8" | 8'-5 3/4" |
| 2.340 m | 2.585 m |
| 30,480 kg | 4,870 kg | 25,610 kg | **CU.M** | **CU.FT** |
| 86 | 3,040 |
| **Purpose** |
| Captioned units can be coordinated from EISU 804001~EISU 804500 and EMCU 801001~EMCU 80250. |

|  |  |
| --- | --- |
| **Exterior** | 45sh |
| Length | Width | Height |
| 45'-0" | 8'-0" | 9'-6" |
| 13.716 m | 2.438 m | 2.896 m |
| **Interior** |
| Length | Width | Height |
| 44'-5 7/10'' | 7'-8 19/32'' | 8'-10 17/64'' |
| 13.556 m | 2.352 m | 2.698 m |
| **Weight** | **Door Opening** |
| MGW | TARE | NET | Width | Height |
| 71,650 lb | 10,360 lb | 61,290 lb | 7'-8" | 8'-6" |
| 2.340 m | 2.585 m |
| 32,500 kg | 4,700 kg | 27,800 kg | **CU.M** | **CU.FT** |
| 86 | 3,040 |
| **Purpose** |
| Captioned units can be coordinated from EISU 802001~EISU 804000. |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |

 |

 |
|

|  |
| --- |
|  |
| **http://www.evergreen-marine.com/tuf1/images/item1.gif** | **Refrigerated Container** |
|  |

|  |  |
| --- | --- |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' M.G.S.S. Refrigerated Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 20reefer |
| Length | Width | Height |
| 20'-0" | 8'-0" | 8'-6" |
| 6.058 m | 2.438 m | 2.591 m |
| **Interior** |
| Length | Width | Height |
| 18'- 17/32" | 7'-6 15/32" | 7'-5 39/54" |
| 5.500 m | 2.298 m | 2.276 m |
| **Nominal** | **Weight** |
| Cubic Capacity | MGW | TARE |
| 1,016 cu.ft. | 67,180 lb | 6,700 lb |
| 28.8 cu.m. | 30,480 kg | 3,020 kg |
| **Cooling capacity** | **Air exchange rate** | **Type** | **Temp.control precision** |
| w(kcal)/C(F) | CFM | cu.m/hr |
| 11,000(9,460)/1.7(35)6,280(5,400)/-18(0) | 0-106 | 0-180 | MHICPE14-2BAIIIEU | +-0.25C |
| 10,550(9,073)/2(35)6,150(5,289)/-18(0) | 0-142 | 0-240 | CARRIER69NT40-551-501 | +-0.25C |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' Aluminum Refrigerated Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 20reefer |
| Length | Width | Height |
| 20'-0" | 8'-0" | 8'-6" |
| 6.058 m | 2.438 m | 2.591 m |
| **Interior** |
| Length | Width | Height |
| 17'-0" | 7'-6" | 7'-3" |
| 5.480 m | 2.286 m | 2.235 m |
| **Nominal** | **Weight** |
| Cubic Capacity | MGW | TARE |
| 989 cu.ft. | 52,800 lb | 6,170 lb |
| 28 cu.m. | 24,000 kg | 2,800 kg |
| **Cooling capacity** | **Air exchange rate** | **Type** | **Temp.control precision** |
| w(kcal)/C(F) | CFM | cu.m/hr |
| 11,000(9,460)/1.7(35)6,280(5,400)/-18(0) | 0-106 | 0-180 | MHICPE14-2BAIIIEU | +-0.25C |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' M.G.S.S. Hi-Cube Refrigerated Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 40reefer |
| Length | Width | Height |
| 40'-0" | 8'-0" | 9'-6" |
| 12.192 m | 2.438 m | 2.896 m |
| **Interior** |
| Length | Width | Height |
| 37'-11 55/64" | 7'-6 15/32" | 8'-4 5/32" |
| 11.585 m | 2.290 m | 2.544 m |
| **Nominal** | **Weight** |
| Cubic Capacity | MGW | TARE |
| 2,384 cu.ft. | 74,960 lb | 10,490 lb |
| 67.5 cu.m. | 34,000 kg | 4,760 kg |
| **Cooling capacity** | **Air exchange rate** | **Type** | **Temp.control precision** |
| w(kcal)/C(F) | CFM | cu.m/hr |
| 11,000(9,460)/1.7(35)6,280(5,400)/-18(0) | 0-106 | 0-180 | MHICPE16-2BAIIIEV | +-0.25C |
| 10,550(9,073)/2(35)6,150(5,289)/-18(0) | 0-142 | 0-240 | CARRIER69NT40-551-501 | +-0.25C |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Hi-Cube Aluminum Refrigerated Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 40rf0 |
| Length | Width | Height |
| 40'-0" | 8'-0" | 9'-6" |
| 12.192 m | 2.438 m | 2.896 m |
| **Interior** |
| Length | Width | Height |
| 37'-11" | 7'-6" | 8'-2" |
| 11.563 m | 2.286 m | 2.507 m |
| **Nominal** | **Weight** |
| Cubic Capacity | MGW | TARE |
| 2,340 cu.ft. | 67,200 lb | 9,480 lb |
| 66.27 cu.m. | 30,480 kg | 4,300 kg |
| **Cooling capacity** | **Air exchange rate** | **Type** | **Temp.control precision** |
| CFM | cu.m/hr | w(kcal)/C(F) |
| 11,000(9,460)/1.7(35)6,280(5,400)/-18(0) | 0-106 | 0-180 | MHICPE14-2BAIIIA/ES | +-0.25C |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |

 |

 |
|

|  |
| --- |
|  |
| **http://www.evergreen-marine.com/tuf1/images/item1.gif** | **Special Container** |
|  |

|  |  |
| --- | --- |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' Full Height Open Top Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 20fhot2 |
| Length | Width | Height |
| 20'-0" | 8'-0" | 8'-6" |
| 6.058 m | 2.438 m | 2.591 m |
| **Interior** |
| Length | Width | Height |
| 19'-4" | 7'-8 1/2" | 7'-8 1/8" |
| 5.898 m | 2.352 m | 2.342 m |
| **Weight** |
| MGW | TARE | NET |
| 44,800 lb | 4,850 lb | 39,950 lb |
| 20,320 kg | 2,200 kg | 18,120 kg |
| **CU.M** | **CU.FT** |
| 32.5 | 1,148 |
| **Purpose** |
| Captioned units can be coordinated from UGMU 490001~UGMU 490150, EMCU 460261~EMUC 460520 and EISU 460001~EISU 460400. |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20 ' Flat Rack Container with Four Freestanding Posts**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 20fccn |
| Length | Width | Height |
| 20'-0" | 8'-0" | 8'-6" |
| 6.058 m | 2.438 m | 2.591 m |
| **Interior** |
| Length | Width | Height |
| 18'-6 7/16" | 6'-7 59/64" | 6'-9 39/64" |
| 5.650 m | 2.030 m | 2.073 m |
| **Weight** |
| MGW | TARE | NET |
| 66,140 lb | 6,150 lb | 59,990 lb |
| 30,000 kg | 2,790 kg | 27,210 kg |
| **Purpose** |
| Captioned units can be coordinated from EMCU 760321~EMCU 760520. |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' Flat Rack Container with Collapsible End**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 20fccn |
| Length | Width | Height |
| 20'-0" | 8'-0" | 8'-6" |
| 6.058 m | 2.438 m | 2.591 m |
| **Interior** |
| Length | Width | Height |
| 18'-5 62/64" | 7'-3 46/64" | 7'-3 59/64" |
| 5.638 m | 2.228 m | 2.233 m |
| **Weight** |
| MGW | TARE | NET |
| 74,950 lb | 6,370 lb | 68,580 lb |
| 34,000 kg | 2,890 kg | 31,110 kg |
| **Purpose** |
| Captioned units can be coordinated from EISU 750000 to EISU 750300. |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' Fuel Tank Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 40fhot1 |
| Length | Width | Height |
| 20'-0" | 8'-0" | 8'-6" |
| 6.058 m | 2.438 m | 2.591 m |
| **Weight** |
| MGW | TARE | NET |
| 36,000 kg | 3,385 kg | 32,615 kg |
| **Capacity** | **Design Temp.**  |
| 24,000 litres  | -20°C to 130°C |
| **Purpose** |
|

|  |
| --- |
| Captioned units can be coordinated from EISU 8010010 to EISU 8010453, and are need for power pack generators equipped on group vessels, not for export or import purpose.  |

 |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' Power Pack Generator Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 40fhot1 |
| Length | Width | Height |
| 20'-0" | 8'-0" | 8'-6" |
| 6.058 m | 2.438 m | 2.591 m |
| **Interior** |
| Length | Width | Height |
| 19'-4 13/16" | 7'-8 19/32" | 7'-9 57/64" |
| 5.898 m | 2.352 m | 2.385 m |
| **Weight** |
| MGW | TARE | MACHINE |
| 8,500 kg | 2,400 kg | 6,100 kg |
| **Power Supply** | **Socket** |
| 450 kw  | 40 |
| **Purpose** |
| Captioned units can be coordinated from EMCU 0000013 to EMCU 0000409. |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Flat Rack Container with Four Freestanding Posts**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 40fccn |
| Length | Width | Height |
| 40'-0" | 8'-0" | 8'-6" |
| 12.192 m | 2.438 m | 2.591 m |
| **Interior** |
| Length | Width | Height |
| 38'-7 15/16" | 6'-7 59/64" | 6'-4 1/2" |
| 11.784 m | 2.030 m | 1.943 m |
| **Weight** |
| MGW | TARE | NET |
| 99,210 lb | 11,908 lb | 87,302 lb |
| 45,000 kg | 5,400 kg | 39,600 kg |
| **Purpose** |
| Captioned units can be coordinated from UGMU 707001~UGMU 707050; EMCU 700251~EMCU 700450. |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Flat Rack Container with Collapsible End**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 40fccn |
| Length | Width | Height |
| 40'-0" | 8'-0" | 8'-6" |
| 12.192 m | 2.438 m | 2.591 m |
| **Interior** |
| Length | Width | Height |
| 38'-7 39/64" | 7'-3 46/64" | 6'-4 61/64" |
| 11.776 m | 2.228 m  | 1.955 m  |
| **Weight** |
| MGW | TARE | NET |
| 99,210 lb | 10,140 lb | 89,070 lb |
| 45,000 kg | 4,600 kg | 40,400 kg |
| **Purpose** |
| Captioned units can be coordinated from EISU 710000~EISU 710500, EMCU 700451~EMCU 700650 |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Flat Rack Hi-Cube Container** |
|   |

|  |  |
| --- | --- |
| **Exterior** | 40hfc |
| Length | Width | Height |
| 40'-0" | 8'-0" | 9'-6" |
| 12.192 m | 2.438 m | 2.896 m |
| **Interior** |
| Length | Width | Height |
| 38'-2 3/4" | 7'-9 7/16" | 7'-5 1/8" |
| 11.652 m | 2.374 m | 2.264 m |
| **Weight** |
| MGW | TARE | NET |
| 115,740 lb | 11,460 lb | 104,280 lb |
| 52,500 kg | 5,200 kg | 47,300 kg |
| **Purpose** |
| Captioned units can be coordinated from EMCU700681-700780 |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Full Height Open Top Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 40fhop |
| Length | Width | Height |
| 40'-0" | 8'-0" | 8'-6" |
| 12.192 m | 2.438 m | 2.591 m |
| **Interior** |
| Length | Width | Height |
| 39'-5" | 7'-8 1/2" | 7'-8 1/8" |
| 12.034 m | 2.352 m | 2.330 m |
| **Weight** |
| MGW | TARE | NET |
| 67,200 lb | 9,040 lb | 58,160 lb |
| 30,480 kg | 4,100 kg | 26,380 kg |
| **CU.M** | **CU.FT** |
| 65.9 | 2,327 |
| **Purpose** |
| Captioned units can be coordinated from EMCU 400362~EMCU 400810,UGMU 407001~UGMU 407050 and EISU 400001~EISU 400600.  |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Hi-Cube Open Top Container** |
|   |

|  |  |
| --- | --- |
| **Exterior** | 40hop |
| Length | Width | Height |
| 40'-0" | 8'-0" | 9'-6" |
| 12.192 m | 2.438 m | 2.896 m |
| **Interior** |
| Length | Width | Height |
| 39'-6" | 7'-9" | 8'-8 7/16" |
| 12.032 m | 2.352 m | 2.653 m |
| **Weight** |
| MGW | TARE | NET |
| 67,200 lb | 9,390 lb | 57,810 lb |
| 30,480 kg | 4,260 kg | 26,220 kg |
| **CU.M** | **CU.FT** |
| 75.1 | 2,650 |
| **Purpose** |
| Captioned units can be coordinated from EMCU400911-401010 |

|  |
| --- |
| http://www.evergreen-marine.com/tuf1/images/top.gif |

 |
| **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Hi-Cube Hanger Container**  |
|   |

|  |  |
| --- | --- |
| **Exterior** | 40sh |
| Length | Width | Height |
| 40'-0" | 8'-0" | 9'-6" |
| 12.19 m | 2.44 m | 2.90 m |
| **Interior** |
| Length | Width | Height |
| 39'-5 45/64" | 7'-8 19/32" | 8'-9 15/16" |
| 12.03 m | 2.35 m | 2.69 m |
| **Weight** | **Door Opening** |
| MGW | TARE | NET | Width | Height |
| 67,200 lb | 9,172 lb | 58,028 lb | 7'-8 1/8" | 8'-5 49/64" |
| 30,480 kg | 4,200 kg | 26,280 kg | 2.343 m | 2.585 m |
| **Purpose** |
| Used for all kinds of garment. |

 |

 |

 |