|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  | | --- | --- | |  | | | **http://www.evergreen-marine.com/tuf1/images/item1.gif** | **Dry Cargo Container** | |  | |  |  | | --- | --- | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' Steel Dry Cargo Container** | |  | |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Exterior** | | | 20sd | | | Length | Width | Height | | 20'-0" | 8'-0" | 8'-6" | | 6.058 m | 2.438 m | 2.591 m | | **Interior** | | | | Length | Width | Height | | 19'-4 13/16" | 7'-8 19/32" | 7'-9 57/64" | | 5.898 m | 2.352 m | 2.385 m | | **Weight** | | | **Door Opening** | | | MGW | TARE | NET | Width | Height | | 52,910 lb | 5,140 lb | 47,770 lb | 7'-8 1/8" | 7'-5 3/4" | | 67,200 lb | 5,290 lb | 61,910 lb | 2.343 m | 2.280 m | | 24,000 kg | 2,330 kg | 21,670 kg | **CU.M** | **CU.FT** | | 30,480 kg | 2,400 kg | 28,080 kg | 33.1 | 1,169 | | **Purpose** | | | | | | 1.Captioned units(MGW 30,480 KG) can be coordinated from EMCU 3204073 and EISU 3568118. 2.Used for all kinds of general cargo. | | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Steel Dry Cargo Container** | |  | |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Exterior** | | | 40sd | | | Length | Width | Height | | 40'-0" | 8'-0" | 8'-6" | | 12.192 m | 2.438 m | 2.591 m | | **Interior** | | | | Length | Width | Height | | 39'-5 45/64" | 7'-8 19/32" | 7'-9 57/64" | | 12.032 m | 2.352 m | 2.385 m | | **Weight** | | | **Door Opening** | | | MGW | TARE | NET | Width | Height | | 67,200 lb | 8,820 lb | 58,380 lb | 7'-8 1/8" | 7'-5 3/4" | | 2.343 m | 2.280 m | | 30,480 kg | 4,000 kg | 26,480 kg | **CU.M** | **CU.FT** | | 67.5 | 2,385 | | **Purpose** | | | | | | Used for all kinds of general cargo. | | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Hi-Cube Steel Dry Cargo Container** | |  | |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Exterior** | | | 40sh | | | Length | Width | Height | | 40'-0" | 8'-0" | 9'-6" | | 12.192 m | 2.438 m | 2.896 m | | **Interior** | | | | Length | Width | Height | | 39'-5 45/64" | 7'-8 19/32" | 8'-9 15/16" | | 12.032 m | 2.352 m | 2.69 m | | **Weight** | | | **Door Opening** | | | MGW | TARE | NET | Width | Height | | 67,200 lb | 9,260 lb | 57,940 lb | 7'-8 1/8" | 8'-5 49/64" | | 2.343 m | 2.585 m | | 30,480 kg | 4,200 kg | 26,280 kg | **CU.M** | **CU.FT** | | 76.2 | 2,690 | | **Purpose** | | | | | | Used for all kinds of general cargo. | | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **45' Hi-Cube Steel Dry Cargo Container** | |  | |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Exterior** | | | 45sh | | | Length | Width | Height | | 45'-0" | 8'-0" | 9'-6" | | 13.716 m | 2.438 m | 2.896 m | | **Interior** | | | | Length | Width | Height | | 44'-5 7/10'' | 7'-8 19/32'' | 8'-10 17/64'' | | 13.556 m | 2.352 m | 2.698 m | | **Weight** | | | **Door Opening** | | | MGW | TARE | NET | Width | Height | | 67,200 lb | 10,580 lb | 56,620 lb | 7'-8 1/8" | 8'-5 3/4" | | 2.340 m | 2.585 m | | 30,480 kg | 4,800 kg | 25,680 kg | **CU.M** | **CU.FT** | | 86.1 | 3,040 | | **Purpose** | | | | | | Used for all kinds of general cargo. | | | | |  |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Exterior** | | | 45sh | | | Length | Width | Height | | 45'-0" | 8'-0" | 9'-6" | | 13.716 m | 2.438 m | 2.896 m | | **Interior** | | | | Length | Width | Height | | 44'-5 7/10'' | 7'-8 19/32'' | 8'-10 17/64'' | | 13.556 m | 2.352 m | 2.698 m | | **Weight** | | | **Door Opening** | | | MGW | TARE | NET | Width | Height | | 67,200 lb | 10,858 lb | 56,342 lb | 7'-8 1/8" | 8'-5 3/4" | | 2.340 m | 2.585 m | | 30,480 kg | 4,870 kg | 25,610 kg | **CU.M** | **CU.FT** | | 86 | 3,040 | | **Purpose** | | | | | | Captioned units can be coordinated from EISU 804001~EISU 804500 and EMCU 801001~EMCU 80250. | | | | |  |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Exterior** | | | 45sh | | | Length | Width | Height | | 45'-0" | 8'-0" | 9'-6" | | 13.716 m | 2.438 m | 2.896 m | | **Interior** | | | | Length | Width | Height | | 44'-5 7/10'' | 7'-8 19/32'' | 8'-10 17/64'' | | 13.556 m | 2.352 m | 2.698 m | | **Weight** | | | **Door Opening** | | | MGW | TARE | NET | Width | Height | | 71,650 lb | 10,360 lb | 61,290 lb | 7'-8" | 8'-6" | | 2.340 m | 2.585 m | | 32,500 kg | 4,700 kg | 27,800 kg | **CU.M** | **CU.FT** | | 86 | 3,040 | | **Purpose** | | | | | | Captioned units can be coordinated from EISU 802001~EISU 804000. | | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | |
| |  |  | | --- | --- | |  | | | **http://www.evergreen-marine.com/tuf1/images/item1.gif** | **Refrigerated Container** | |  | |  |  | | --- | --- | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' M.G.S.S. Refrigerated Container** | |  | |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Exterior** | | | 20reefer | | | Length | Width | Height | | 20'-0" | 8'-0" | 8'-6" | | 6.058 m | 2.438 m | 2.591 m | | **Interior** | | | | Length | Width | Height | | 18'- 17/32" | 7'-6 15/32" | 7'-5 39/54" | | 5.500 m | 2.298 m | 2.276 m | | **Nominal** | | | **Weight** | | | Cubic Capacity | | | MGW | TARE | | 1,016 cu.ft. | | | 67,180 lb | 6,700 lb | | 28.8 cu.m. | | | 30,480 kg | 3,020 kg | | **Cooling capacity** | **Air exchange rate** | | **Type** | **Temp. control precision** | | w(kcal)/C(F) | CFM | cu.m/hr | | 11,000(9,460)/1.7(35) 6,280(5,400)/-18(0) | 0-106 | 0-180 | MHI CPE14-2BAIIIEU | +-0.25C | | 10,550(9,073)/2(35) 6,150(5,289)/-18(0) | 0-142 | 0-240 | CARRIER 69NT40-551-501 | +-0.25C |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' Aluminum Refrigerated Container** | |  | |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Exterior** | | | 20reefer | | | Length | Width | Height | | 20'-0" | 8'-0" | 8'-6" | | 6.058 m | 2.438 m | 2.591 m | | **Interior** | | | | Length | Width | Height | | 17'-0" | 7'-6" | 7'-3" | | 5.480 m | 2.286 m | 2.235 m | | **Nominal** | | | **Weight** | | | Cubic Capacity | | | MGW | TARE | | 989 cu.ft. | | | 52,800 lb | 6,170 lb | | 28 cu.m. | | | 24,000 kg | 2,800 kg | | **Cooling capacity** | **Air exchange rate** | | **Type** | **Temp. control precision** | | w(kcal)/C(F) | CFM | cu.m/hr | | 11,000(9,460)/1.7(35) 6,280(5,400)/-18(0) | 0-106 | 0-180 | MHI CPE14-2BAIIIEU | +-0.25C |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' M.G.S.S. Hi-Cube Refrigerated Container** | |  | |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Exterior** | | | 40reefer | | | Length | Width | Height | | 40'-0" | 8'-0" | 9'-6" | | 12.192 m | 2.438 m | 2.896 m | | **Interior** | | | | Length | Width | Height | | 37'-11 55/64" | 7'-6 15/32" | 8'-4 5/32" | | 11.585 m | 2.290 m | 2.544 m | | **Nominal** | | | **Weight** | | | Cubic Capacity | | | MGW | TARE | | 2,384 cu.ft. | | | 74,960 lb | 10,490 lb | | 67.5 cu.m. | | | 34,000 kg | 4,760 kg | | **Cooling capacity** | **Air exchange rate** | | **Type** | **Temp. control precision** | | w(kcal)/C(F) | CFM | cu.m/hr | | 11,000(9,460)/1.7(35) 6,280(5,400)/-18(0) | 0-106 | 0-180 | MHI CPE16-2BAIIIEV | +-0.25C | | 10,550(9,073)/2(35) 6,150(5,289)/-18(0) | 0-142 | 0-240 | CARRIER 69NT40-551-501 | +-0.25C |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Hi-Cube Aluminum Refrigerated Container** | |  | |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Exterior** | | | 40rf0 | | | Length | Width | Height | | 40'-0" | 8'-0" | 9'-6" | | 12.192 m | 2.438 m | 2.896 m | | **Interior** | | | | Length | Width | Height | | 37'-11" | 7'-6" | 8'-2" | | 11.563 m | 2.286 m | 2.507 m | | **Nominal** | | | **Weight** | | | Cubic Capacity | | | MGW | TARE | | 2,340 cu.ft. | | | 67,200 lb | 9,480 lb | | 66.27 cu.m. | | | 30,480 kg | 4,300 kg | | **Cooling capacity** | **Air exchange rate** | | **Type** | **Temp. control precision** | | CFM | cu.m/hr | w(kcal)/C(F) | | 11,000(9,460)/1.7(35) 6,280(5,400)/-18(0) | 0-106 | 0-180 | MHI CPE14-2BAIIIA/ES | +-0.25C |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | |
| |  |  | | --- | --- | |  | | | **http://www.evergreen-marine.com/tuf1/images/item1.gif** | **Special Container** | |  | |  |  | | --- | --- | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' Full Height Open Top Container** | |  | |  |  |  |  | | --- | --- | --- | --- | | **Exterior** | | | 20fhot2 | | Length | Width | Height | | 20'-0" | 8'-0" | 8'-6" | | 6.058 m | 2.438 m | 2.591 m | | **Interior** | | | | Length | Width | Height | | 19'-4" | 7'-8 1/2" | 7'-8 1/8" | | 5.898 m | 2.352 m | 2.342 m | | **Weight** | | | | MGW | TARE | NET | | 44,800 lb | 4,850 lb | 39,950 lb | | 20,320 kg | 2,200 kg | 18,120 kg | | **CU.M** | | | **CU.FT** | | 32.5 | | | 1,148 | | **Purpose** | | | | | Captioned units can be coordinated from UGMU 490001~UGMU 490150, EMCU 460261~EMUC 460520 and  EISU 460001~EISU 460400. | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20 ' Flat Rack Container with Four Freestanding Posts** | |  | |  |  |  |  | | --- | --- | --- | --- | | **Exterior** | | | 20fccn | | Length | Width | Height | | 20'-0" | 8'-0" | 8'-6" | | 6.058 m | 2.438 m | 2.591 m | | **Interior** | | | | Length | Width | Height | | 18'-6 7/16" | 6'-7 59/64" | 6'-9 39/64" | | 5.650 m | 2.030 m | 2.073 m | | **Weight** | | | | MGW | TARE | NET | | 66,140 lb | 6,150 lb | 59,990 lb | | 30,000 kg | 2,790 kg | 27,210 kg | | **Purpose** | | | | | Captioned units can be coordinated from EMCU 760321~EMCU 760520. | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' Flat Rack Container with Collapsible End** | |  | |  |  |  |  | | --- | --- | --- | --- | | **Exterior** | | | 20fccn | | Length | Width | Height | | 20'-0" | 8'-0" | 8'-6" | | 6.058 m | 2.438 m | 2.591 m | | **Interior** | | | | Length | Width | Height | | 18'-5 62/64" | 7'-3 46/64" | 7'-3 59/64" | | 5.638 m | 2.228 m | 2.233 m | | **Weight** | | | | MGW | TARE | NET | | 74,950 lb | 6,370 lb | 68,580 lb | | 34,000 kg | 2,890 kg | 31,110 kg | | **Purpose** | | | | | Captioned units can be coordinated from EISU 750000 to EISU 750300. | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' Fuel Tank Container** | |  | |  |  |  |  | | --- | --- | --- | --- | | **Exterior** | | | 40fhot1 | | Length | Width | Height | | 20'-0" | 8'-0" | 8'-6" | | 6.058 m | 2.438 m | 2.591 m | | **Weight** | | | | MGW | TARE | NET | | 36,000 kg | 3,385 kg | 32,615 kg | | **Capacity** | | | **Design Temp.** | | 24,000 litres | | | -20°C to 130°C | | **Purpose** | | | | | |  | | --- | | Captioned units can be coordinated from EISU 8010010 to EISU 8010453, and  are need for power pack generators equipped on group vessels, not for export or import purpose. | | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **20' Power Pack Generator Container** | |  | |  |  |  |  | | --- | --- | --- | --- | | **Exterior** | | | 40fhot1 | | Length | Width | Height | | 20'-0" | 8'-0" | 8'-6" | | 6.058 m | 2.438 m | 2.591 m | | **Interior** | | | | Length | Width | Height | | 19'-4 13/16" | 7'-8 19/32" | 7'-9 57/64" | | 5.898 m | 2.352 m | 2.385 m | | **Weight** | | | | MGW | TARE | MACHINE | | 8,500 kg | 2,400 kg | 6,100 kg | | **Power Supply** | | | **Socket** | | 450 kw | | | 40 | | **Purpose** | | | | | Captioned units can be coordinated from EMCU 0000013 to EMCU 0000409. | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Flat Rack Container with Four Freestanding Posts** | |  | |  |  |  |  | | --- | --- | --- | --- | | **Exterior** | | | 40fccn | | Length | Width | Height | | 40'-0" | 8'-0" | 8'-6" | | 12.192 m | 2.438 m | 2.591 m | | **Interior** | | | | Length | Width | Height | | 38'-7 15/16" | 6'-7 59/64" | 6'-4 1/2" | | 11.784 m | 2.030 m | 1.943 m | | **Weight** | | | | MGW | TARE | NET | | 99,210 lb | 11,908 lb | 87,302 lb | | 45,000 kg | 5,400 kg | 39,600 kg | | **Purpose** | | | | | Captioned units can be coordinated from UGMU 707001~UGMU 707050; EMCU 700251~EMCU 700450. | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Flat Rack Container with Collapsible End** | |  | |  |  |  |  | | --- | --- | --- | --- | | **Exterior** | | | 40fccn | | Length | Width | Height | | 40'-0" | 8'-0" | 8'-6" | | 12.192 m | 2.438 m | 2.591 m | | **Interior** | | | | Length | Width | Height | | 38'-7 39/64" | 7'-3 46/64" | 6'-4 61/64" | | 11.776 m | 2.228 m | 1.955 m | | **Weight** | | | | MGW | TARE | NET | | 99,210 lb | 10,140 lb | 89,070 lb | | 45,000 kg | 4,600 kg | 40,400 kg | | **Purpose** | | | | | Captioned units can be coordinated from EISU 710000~EISU 710500, EMCU 700451~EMCU 700650 | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Flat Rack Hi-Cube Container** | |  | |  |  |  |  | | --- | --- | --- | --- | | **Exterior** | | | 40hfc | | Length | Width | Height | | 40'-0" | 8'-0" | 9'-6" | | 12.192 m | 2.438 m | 2.896 m | | **Interior** | | | | Length | Width | Height | | 38'-2 3/4" | 7'-9 7/16" | 7'-5 1/8" | | 11.652 m | 2.374 m | 2.264 m | | **Weight** | | | | MGW | TARE | NET | | 115,740 lb | 11,460 lb | 104,280 lb | | 52,500 kg | 5,200 kg | 47,300 kg | | **Purpose** | | | | | Captioned units can be coordinated from EMCU700681-700780 | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Full Height Open Top Container** | |  | |  |  |  |  | | --- | --- | --- | --- | | **Exterior** | | | 40fhop | | Length | Width | Height | | 40'-0" | 8'-0" | 8'-6" | | 12.192 m | 2.438 m | 2.591 m | | **Interior** | | | | Length | Width | Height | | 39'-5" | 7'-8 1/2" | 7'-8 1/8" | | 12.034 m | 2.352 m | 2.330 m | | **Weight** | | | | MGW | TARE | NET | | 67,200 lb | 9,040 lb | 58,160 lb | | 30,480 kg | 4,100 kg | 26,380 kg | | **CU.M** | | | **CU.FT** | | 65.9 | | | 2,327 | | **Purpose** | | | | | Captioned units can be coordinated from EMCU 400362~EMCU 400810, UGMU 407001~UGMU 407050 and EISU 400001~EISU 400600. | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Hi-Cube Open Top Container** | |  | |  |  |  |  | | --- | --- | --- | --- | | **Exterior** | | | 40hop | | Length | Width | Height | | 40'-0" | 8'-0" | 9'-6" | | 12.192 m | 2.438 m | 2.896 m | | **Interior** | | | | Length | Width | Height | | 39'-6" | 7'-9" | 8'-8 7/16" | | 12.032 m | 2.352 m | 2.653 m | | **Weight** | | | | MGW | TARE | NET | | 67,200 lb | 9,390 lb | 57,810 lb | | 30,480 kg | 4,260 kg | 26,220 kg | | **CU.M** | | | **CU.FT** | | 75.1 | | | 2,650 | | **Purpose** | | | | | Captioned units can be coordinated from EMCU400911-401010 | | | | |      |  | | --- | | [http://www.evergreen-marine.com/tuf1/images/top.gif](http://www.evergreen-marine.com/tei1/jsp/TEI1_Containers.jsp#top) | | | **http://www.evergreen-marine.com/tuf1/images/item2.gif** | **40' Hi-Cube Hanger Container** | |  | |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Exterior** | | | 40sh | | | Length | Width | Height | | 40'-0" | 8'-0" | 9'-6" | | 12.19 m | 2.44 m | 2.90 m | | **Interior** | | | | Length | Width | Height | | 39'-5 45/64" | 7'-8 19/32" | 8'-9 15/16" | | 12.03 m | 2.35 m | 2.69 m | | **Weight** | | | **Door Opening** | | | MGW | TARE | NET | Width | Height | | 67,200 lb | 9,172 lb | 58,028 lb | 7'-8 1/8" | 8'-5 49/64" | | 30,480 kg | 4,200 kg | 26,280 kg | 2.343 m | 2.585 m | | **Purpose** | | | | | | Used for all kinds of garment. | | | | | | | |