WALL REPAIR GUIDE

**Issue. WHITE** block walls directly facing a sidewalk and or street, NOT the walls between homes, not in compliance with HOA CC&R's. The types of defects/damages are as follows:

1 - Holes or other actual deterioration/crumbling/erosion of cinder block 2 - Efflorescence and or stains on the walls

3 - Discoloration of paint

**Goal.** Timely completion/remedy of defects/damages while consistent in color.

**Responsibility**. Per CC&R section 11.14. It is the respective homeowner’s responsibility to maintain and repair walls as originally constructed, all at such Owners sole cost and expense.

**Wall must be pressure washed before applying stain.**

# Option 1 No crumbling/erosion of the block wall stained or showing Efflorescence

1. Short-term – Pressure wash and Stain (Steps in order)
   1. Pressure/Power wash with TSP entire perimeter wall - top to bottom
   2. Allow at least 72 hours drying time after power wash before proceeding to next step
   3. Stain entire perimeter wall**. (Color must be Sherwin-Williams INCREDIBLE WHITE stain).** Recommended product is **H & C Colortop concrete stain Product Number 20-101214 tinted to SW 7028.** Follow manufacturer recommendations on temperatures when staining.

.

# Option 2 Wall surface is eroded/crumbling/deteriorated or contains holes

1. Short-term – Pressure wash, repair Damage and Stain (Steps in order)
   1. Pressure/Power wash with TSP entire perimeter wall - top to bottom
   2. Allow at least 72 hours drying time after power wash before proceeding to next step
   3. If holes or any deterioration/crumbling/erosion; a hydraulic concrete substance must be smoothly applied to achieve uniform surface
   4. Apply mortar to smooth out
   5. Retain grout lines when doing this.
   6. Stain entire perimeter wall**. (Color must be Sherwin-Williams INCREDIBLE WHITE stain).** Recommended product is **H & C Colortop concrete stain Product Number 20-101214 tinted to SW 7028.** Follow manufacturer recommendations on temperatures when staining.

**Optional.** One-inch weep holes may be drilled at base of wall every 2 – 3 feet to allow drainage.

# NOTE: ALL perimeter walls MUST be stained the exact same color. No exception. Option 3 Delay serious damage

1. Long -term – Trench inside wall (Steps in order)
   1. Dig trench down to footing and 2 feet wide the entire length of the inside surface of the wall (see variables)
   2. Seal the entire inside surface of the wall
   3. One-inch weep holes should be drilled at base of wall every 2 – 3 feet to allow drainage.
   4. Apply Xypex or Sealant product for cinder block walls on inside of wall
   5. Refill trench with ½ to 1-inch gravel
   6. Outside of wall **Follow appropriate Option 1 or Option 2**

# Variables.

1. If any sprinklers, trees, concrete surfaces, caliche etc. are in the way, they need to be removed
2. Variables. Any other drainage related issues should be resolved - to industry standards

# Root causes of damage

1. Trees and shrubs planted within 5 feet of the wall
2. Over watering

This information is for general information purposes only. We make no representations or warranties of any kind, express or implied, about the completeness, accuracy, reliability, suitability, or availability with respect to the information, products, costs or services for any purpose. Any reliance you place on such information is strictly at your own risk. You are advised to consult an expert with respect to these matters.