{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Application Data","Drop Downs"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Application Data","index":0,"n_rows":51,"n_cols":14,"rows_kept":51,"cut":false,"hidden":false,"merged":[[50,11,52,14],[49,11,49,14],[34,11,34,14],[35,11,35,12],[35,13,35,14],[27,0,27,14],[36,0,36,14],[37,11,37,14],[38,11,38,14],[39,11,39,12],[39,13,39,14],[9,11,9,14],[14,4,14,6],[10,4,10,7],[10,8,10,10],[10,11,10,12],[41,13,41,14],[46,11,46,14],[47,11,47,14],[18,4,18,6],[18,8,18,9],[45,8,45,9],[19,0,19,14],[21,11,21,12],[22,11,22,12],[22,13,22,14],[23,11,23,12],[24,4,24,7],[24,8,24,10],[26,4,26,10],[23,4,23,7],[23,8,23,10],[0,11,3,14],[6,11,6,12],[6,13,6,14],[5,11,5,13],[7,11,7,14],[4,11,4,14],[8,0,8,14],[16,4,16,7],[16,8,16,10],[16,11,16,12],[16,13,16,14],[5,4,5,7],[5,8,5,10],[6,4,6,7],[6,8,6,10],[7,4,7,10],[13,4,13,6],[15,4,15,6],[9,4,9,10],[28,11,28,14],[30,11,30,12],[30,13,30,14],[31,11,31,12],[31,13,31,14],[32,11,32,14],[33,11,33,14],[23,13,23,14],[24,11,24,12],[24,13,24,14],[26,11,26,14],[44,9,44,10],[43,4,43,8],[44,4,44,8],[30,8,30,10],[31,4,31,7],[31,8,31,10],[40,4,40,10],[35,8,35,10],[41,4,41,7],[41,8,41,10],[43,9,43,10],[33,4,33,10],[38,4,38,10],[37,4,37,10],[40,11,40,12],[40,13,40,14],[41,11,41,12],[42,8,42,10],[42,11,42,12],[0,0,3,9],[4,0,7,2],[9,0,18,2],[17,8,17,10],[4,4,4,10],[22,8,22,10],[20,0,26,2],[25,4,25,10],[11,4,11,6],[12,4,12,6],[21,4,21,7],[21,9,21,10],[22,4,22,7],[20,4,20,7],[20,9,20,10],[17,4,17,7],[17,11,17,12],[17,13,17,14],[20,11,20,12],[10,13,10,14],[49,0,52,2],[49,4,49,10],[50,3,52,3],[50,4,52,10],[44,11,44,12],[43,13,43,14],[43,11,43,12],[44,13,44,14],[34,4,34,10],[28,0,35,2],[32,4,32,10],[39,4,39,7],[39,8,39,10],[35,4,35,7],[30,4,30,7],[28,4,28,10],[29,4,29,10],[37,0,46,2],[47,4,47,10],[46,4,46,10],[45,4,45,6],[42,4,42,7],[42,13,42,14]]}
[null,null,null,null,null,null,null,null,null,null,null,"Liquid Flowmeter\nApplication Data Sheet\nHighlighed Row = Mandatory Field (Rev 1.5)"]
[]
[]
[]
["GENERAL",null,null,1,"Company Name "]
[null,null,null,2,"Contact Name",null,null,null,"Date"]
[null,null,null,3,"Phone",null,null,null,"Email"]
[null,null,null,4,"Address"]
[]
["PROCESS CONDITIONS",null,null,5,"Tag Number"]
[null,null,null,6,"Fluid",null,null,null,"Stream Composition"]
[null,null,null,7,"Flow",null,null,"Min.","Oper.","Max.","Units"]
[null,null,null,8,"Temp",null,null,"Min.","Oper.","Max.","Units"]
[null,null,null,9,"Pressure",null,null,"Min.","Oper.","Max.","Units"]
[null,null,null,10,"Density",null,null,"Min.","Oper.","Max.","Units"]
[null,null,null,11,"Viscosity",null,null,"Min.","Oper.","Max.","Units"]
[null,null,null,12,"Corrosive / Abrasive Property.",null,null,null,"Build Up"]
[null,null,null,13,"%Suspended Solids",null,null,null,"% Gas Bubbles"]
[null,null,null,14,"Design Max Press.",null,null,"Units","Design Max.Temp.",null,"Units"]
[]
["PIPING /\nINSTALLATION REQUIREMENTS",null,null,15,"Pipe Material",null,null,null,"Pipe Size","Wall/Schd. "]
[null,null,null,16,"Flange Rating",null,null,null,"Lining","Pipe Spec "]
[null,null,null,17,"Upstream Straight Run",null,null,null,"Downstream",null,null,"(Pipe Diameters)",null,"(Pipe Diameters)"]
[null,null,null,18,"Pipe Orientation",null,null,null,"Clamp-on / Wetted"]
[null,null,null,19,"Flowcell Required",null,null,null,"Transducer Removal"]
[null,null,null,20,"Transducer Haz Area (Type/Zone/Gas Group/T Class)"]
[null,null,null,21,"Ambient Conditions (Temp, Rh%, Marine env., etc.)"]
[]
["ELECTRONICS / MEASUREMENT\nPARAMETERS",null,null,22,"Transmitter Housing Requirement "]
[null,null,null,23,"Electronics Haz Area (Type/Zone/Gas Group/T Class)"]
[null,null,null,24,"Analog Outputs",null,null,null,"Digital Outputs"]
[null,null,null,25,"Inputs",null,null,null,"Alarms"]
[null,null,null,26,"Communications "]
[null,null,null,27,"Power Available"]
[null,null,null,28,"Required Cable Length (1000 ft. Max)"]
[null,null,null,29,"Desired Accuracy",null,null,null,"Desired Repeatability"]
[]
["FLOWCELL ",null,null,30,"Pipe Spec "]
[null,null,null,31,"NDE Required (LPI, Hydro, X-ray are standard)"]
[null,null,null,32,"Material",null,null,null,"Grade"]
[null,null,null,33,"Other Material :Specify Pipe and Flange ",null,null,null,null,null,null,"Pipe:",null,"Flange:"]
[null,null,null,34,"Flange Type",null,null,null,"Pipe Schedule "]
[null,null,null,35,"Flange Rating ",null,null,null,"Flange Series (if pipe>24\")"]
[null,null,null,36,"Addl Port Pressure - Size/Class",null,null,null,null,"Type"]
[null,null,null,37,"Addl Port Temp - Size/Class",null,null,null,null,"Type"]
[null,null,null,38,"Design Max Press.",null,null,"Units","Design Max.Temp.",null,"Units"]
[null,null,null,39,"Paint System"]
[null,null,null,40,"Interior Coating "]
[]
["OTHER ",null,null,41,"Specify any regulatory requirements "]
[null,null,null,42,"NOTES:",null,null,null,null,null,null,"(Specify any special requirements, clearance issues, ect.) "]

{"sheet":"Drop Downs","index":1,"n_rows":62,"n_cols":8,"rows_kept":62,"cut":false,"hidden":true,"merged":[]}
["Measurement location","Flowcell Required?","Isolation Valve","Location","Transducer Haz Area","Transmitter Haz Area","Electronics Housing Requirement "]
["Horizontal Flow","Yes","Provided by BHGE","Hazardous","USA/CAN Div1, Cl1 Gr CD","None, NEMA4X & IP66","Weatherproof, Non-incendive NEMA4X & IP66 (Cl1 Div 2)"]
["Vertical Flow (Up)","No (Hot/Cold Tap)","Provided by Customer ","Nonhazardous","USA/CAN Div1, Cl1 Gr BCD","USA/CAN Div2, Cl1 ABCD","Explosionproof NEMA7 / 4X"]
["Vertical Flow (Down)",null,"None","Nonhazardous Weatherproof","ATEX II 2 G Ex d IIC T6","USA/CAN Div1, Cl1 BCD","Portable "]
["Other (Please Specify)",null,null,null,"IECEx II 2 G Ex d IIC T6","ATEX II 2 G Ex d IIB+H2 T6","Intrinsically Safe "]
[null,null,null,null,"INMETRO","ATEX II 2 G Ex d IIC T6","Other (List Requirments for Other)"]
[null,"Transducer",null,null,"Other (Specify in Notes)","IECEx Ex d IIB+H2 T6"]
[null,"Clamp-On",null,null,"General Purpose Area","IECEx Ex d IIC T6"]
[null,"Wetted ",null,null,null,"INMETRO"]
[null,null,null,null,null,"Other (Specify in Notes)"]
[null,null,null,null,null,"General Purpose Area"]
[]
[]
["Analog Outputs","Digital Outputs","Alarms","Inputs (Pres./Temp)","Power Available","NDE","Communication"]
["Two isolated 4 to 20","None","None","Isolated 4-20 mA","100/120 VAC","X-Ray","RS232"]
["Six isolated 4 to 20","Four config. Pulse total/freq. outputs","Standard alarm relays","RTD","220/240 VAC","LPI","RS485"]
["Ten isolated 4 to 20","Modbus Digital","Hermetically sealed alarms ","Isolated 4-20 mA & RTD","12 to 28 VDC","HydroStatic"]
[null,"Modbus digital + 4 config. Pluse total/freq outputs",null,null,null,"Mag Particle "]
[null,"HART",null,null,null,"PMI"]
[null,"HART + 4 config. Pulse total/freq outputs",null,null,null,"Charpy Impact"]
[null,"MODBUS TCP",null,null,null,"Post Weld Heat Treatment"]
[null,"Ethernet card (panaview/OPC)",null,null,null,"NACE"]
[null,"Foundation Fieldbus",null,null,null,"Brinell Hardness"]
[null,"BACnet over Ethernet",null,null,null,"Others"]
[]
[]
["Carbon Steel","Stainless Steel","5C-1/2M","9C-1/2M","Flange Rating","Flange Type","Flange Type","Flanged/Weld Prep"]
["ASTM A106 GrB/A105 (Valid to 24\" NPS)","ASTM A312 Gr304/A182 GrF304","ASTM A335 GrP5/A182 GrF5","ASTM A335 GrP9/A182 GrF9",150,"Weldneck","ANSI B16.47A","Flanged "]
["ASTM A672GrC70/A105 (Valid > 24\" NPS)","ASTM A312 Gr316/A182 GrF360","Other (Enter Below)","Other (Enter Below)",300,"Slip-on","ANSI B16.47B","Weld-Prep"]
["ASTM A333 Gr6/A350LF2","Other (Enter Below)",null,null,600,"RTJ",null,"Other"]
["Other (Enter Below)",null,null,null,900,"AWWA"]
[null,null,null,null,1500,"Weld Prep"]
[null,null,null,null,2500,"Other (Specify in Notes)"]
["Port Type","Paint System ","Interior Coating ",null,"Other (Specify in Notes)"]
["Thredolet","System A - Bare Metal (Bare Steel, no coating)","Standard Water Soluable Rust Inhibitor "]
["Sockolet","System B -High Temperature Primer (Dry Temp. Resistance: 750oF/399oC)\n(Surface Prep: Surface prep to near white metal SP-10 / Primer Coat: Carbonic 11 Primer, 3-4 mils DFT, Manufacturer's Color Code 0700 (Gray) / Cure per Manufacturer's specifications)","Special (Specify in Notes, Include Coating spec and paint system)",null,"Gas Composition Tab"]
["Nipple","System C - 1 Coat Epoxy Paint, Self Priming (Dry Temp. Resistance: 425oF/218oC)\n(Surface Prep to near white metal SP-10 / Top Coat: Carboline Thermoline 450 Novalak Glass Filled Epoxy / Manufacturer's Color Code : 5742 (Gray), Cure per Manufacturer's specifications / Self Priming, No primer coat needed)","None",null,"Attaching Gas Composition to ADS"]
["Flanged","System D - 2 Coat Silicone Paint (Dry Temp. Resistance: 1000oF/538oC)\n(Surface Prep: Surface prep to near white metal SP-10 / Primer Coat: Carbozinc 11 Primer 3-4 mils DFT / Top Coat: Carboline Thermoline 4700, 2 coat at 1.5 mils DFT each / Manufacturer's Color Code : C901 (Aluminum) / Cure primer and top coats per manufacturer's specifications, then final cure at 400oF/205oC for 2 hours.",null,null,"Fill Out Gas Composition Tab"]
[null,"System E - 2 Coat Silicone Paint (Dry Temp. Resistance: 1000oF/538oC)\n(Surface Prep: Surface prep to near white metal SP-10 / Primer Coat: Carbozinc 11 Primer 3-4 mils DFT / Top Coat: Carboline Thermoline 4700, 2 coat at 1.5 mils DFT each / Manufacturer's Color Code : C901 (Aluminum) / Cure primer and top coats per manufacturer's specifications\nThe final cure for paint system E wil be at the customer site when it is exposed to the actual application temperatures.  Customer should expect/anticipate fumes to be present during initial exposure to elevated temperatures)"]
[null,"None "]
[null,"Special (Specify in Notes, Include Coating Spec and Paint System)"]
[]
["Lining","Pipe Spec","Transducer Removal"]
["Yes (specify in notes)","Yes (attached)","Yes"]
["No","No","No"]
[]
["Hazardous area ratings"]
["FM/CSA","General Purpose","Group C&D","T1"]
["ATEX","Cl1, Div1","Group B,C&D","T2"]
["IECEx","Cl1, Div2","IIA","T3"]
[null,"Zone 0","IIB","T4"]
[null,"Zone 1","IIB+H2","T5"]
[null,"Zone 2","IIC","T6"]
[]
["Temperature","Pressure","Pipe Schedule"]
["°C","PSIG",20]
["°F","Barg",30]
[null,"Mpag",40]
[null,null,"Std"]
[null,null,"XS"]
[null,null,60]
[null,null,80]