**T**ruck **M**ounted **A**ttenuators are now required if you are working on a road with a speed limit of 45 mph or greater.