| East FEliciana Rural Water System 10270 Highway 10  Ethel, Louisiana 70777  225-683-9698 / 225-683-9610 Fax  www.eastfelicianaruralwater.com  **Application for Water Main Extension** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **fOR oFFICE uSE oNLY** | | | | | | | | | |
| Customer#: | | |  | | | | Application Date: | | |
| Location#: | | |  | | | | Receipt#: | | |
| Route / Station#: | | |  | | | | Install Date: | | |
| Work Order#: | | |  | | | | Meter #: | | |
| Turn on Date: | | |  | | | | ERT#: | | |
| Meter Reading: | | |  | | | | Inspected By: | | |
|  | | |  | | | | Lock Out Tag#: | | |
| **APPLICANT INFORMATION** | | | | | | | | | |
| Date:6/3/14 | Time: 1:49 PM | | | | Service Date Requested:1/1/14 | | | | |
| Applicant’s Name: | | | | | | | | | |
| Applicant’s Date of birth: 1/1/14 | | | | Last 4 digit of SSN: 1234 | | | | Driver’s Lic#: 123456789 | |
| Phone#: 225-225-2255 | | | | | | | | | |
| Mailing Address: | | | | | | | | | |
| City: | | | | State: | | | | ZIP Code: | |
| Resident Status: | | | | Have you ever had service with EFRW? | | | | | |
| Email Address: | | | | | | | | | |
| Line Extension Request for Water Usage Purpose:  Type: | | | | | | | | | |
| Parish: | | | | | | | | | |
| Service address: | | | | | | | | | |
| Written Description of Extension Location *(Include number and size of lots to be served)* | | | | | | | | | |
| Federal Requirements | | | | | | | | | |
| The following information is requested by the federal government in order to monitor compliance with federal laws prohibiting discrimination against applicants seeking to participate in this program. You are not required to furnish this information but are encouraged to do so. This will not be used in evaluation of your application, or to discriminate against you in any way. However, if you choose not to furnish it, we are required to note the race national orgin of applicant on the basis of visual observation or surname. | | | | | | | | | |
| Male / Female: | | National Orgin: | | | | Hispanic/ Non-Hispanic: | | | |
| **AUTHORIZATION** | | | | | | | | | |
| I authorize East Feliciana Rural Water System to verify the information provided on this form and further agree to the following terms of the attached *“Water Main Line Extension Policies and Procedures”.* | | | | | | | | | |
| Electronic Signature:  *(To file this application electronically, please enter the last 4 digits of your SS#)*  ***\*\* Copy of Driver’s License is required in order to process application !!*** | | | | | | | | | Date:6/3/2014 |

**EAST FELICIANA RURAL WATER SYSTEM**

**10270 Highway 10**

# ETHEL, LOUISIANA 70730

**(225) 683-9698 FAX (225) 683-9610**

**eastfelicianaruralwater.com**

*“This institution is an equal opportunity provider.”*

The East Feliciana Rural Water System hereby formally amends the formal written policy originally approved on September 21, 2006 on January 24, 2018. On January 24, 2018, the Board of Directors adopted the amended formal written policy regarding new developments within East Feliciana Rural Water’s service area. Any developers or persons requesting service in an undeveloped area should submit a Line Extension Application along with a map representing the proposed development in writing to the East Feliciana Rural Water System’s Board of Directors for consideration. The Board of Directors will base their decision on the attached *“Water Line Extension Criteria”* and compliance with all of the *“Specifications for Line Extension”* requirements being met.

If the proposed development is approved by the Board of Directors for EFWR, the developer will be required to submit the name of the contractor qualified to install the water mains as well as a set of construction plans and specifications sealed by a state licensed engineer for review. The contractor shall be licensed with the state to perform this type of work. These documents must be approved in writing by the EFRWS, as well as, a letter of approval from Louisiana Department of Health & Hospitals.

The contractor will be required to contact the East Feliciana Rural Water System’s Manager to schedule a pre-construction meeting. At the time of the pre-construction meeting the contractor will be require to provide a copy of their license, bond and insurance listing EFRW as additionally insured. At the pre-construction meeting the System Manager will provide “Specifications for Line Extensions, Water Mains Associated Work in Subdivisions and New Development Connecting to the East Feliciana Rural Water System”. East Feliciana Rural Water System will provide a construction inspector during construction to certify that the water mains are installed to specifications. The cost for this inspector shall be borne by the Developer/person requesting service. Additionally, the developer will warranty the new construction for one year upon completion. In the event of an emergency, EFRW reserves the right to perform emergency repairs at the expense of the developer.

New Development tie-ins to East Feliciana Rural Water System’s existing system will be performed by the Contractor and observed by EFRWS personnel. Upon completion of the tie-in, the contractor will be required to super chlorinate, flush and pressure test. Once pressure test has been approved by EFRW, EFRW will sample the new line. Upon written proof of clear health samples, East Feliciana Rural Water System will accept ownership for the new line extension.

**EAST FELICIANA RURAL WATER SYSTEM**

**10270 Highway 10**

# ETHEL, LOUISIANA 70730

**(225) 683-9698 FAX (225) 683-9610**

**eastfelicianaruralwater.com**

*“This institution is an equal opportunity provider.”*

**Specifications for Line Extensions, Water Mains and Associated Work in Subdivisions**

**Connecting to the East Feliciana Rural Water System**

1. Water lines shall be placed in adequate dedicated right of way for maintenance and operations.
2. Any new **Subdivision Developments** must be tied into a 6-inch main or larger.
3. Pipe size requirements for **New Line Extensions (in Non-Subdivisions)** shall be equal to the pipe size currently available in the area. (No smaller than a 3-inch line - subject to approval by EFRWS.)
4. All water mains shall be SDR 26 Class 160 PVC with rubber gasket joint. All mains shall have 12 gauge locator wire.
5. All fittings shall be mechanical joint cement lined ductile iron. This applies to all 90 degree fittings, tees, 45 degree fittings and any fittings in the system. All fittings valves etc. shall be properly restrained.
6. Fire hydrants should be installed off the water main with their own individual 6-inch gate valve coupled to the main line tee with an anchor coupling. The fire hydrant shall be a 5 ¼-inch size and meet AWWA Standard C-502.
7. All creek and drain crossings shall be directional bored with HDPE pipe tied to the water main with Stiffener and M.J. couplings.
8. All 90degree elbows & T’s must have mechanical joint restraints. *(example: Mega Lug)*
9. All water mains shall have a minimum of 30 inches of cover from top of the water main to grade.
10. Water mains and associated work must be inspected by EFRW System personnel during construction and deeded to the East Feliciana Rural Water System upon completion. Cost for these inspections shall be borne by the Developer/person requesting service.
11. All valves furnished and installed shall be resilient seated AWWA gate with cast iron valve boxes. The Valve boxes shall have concrete 4-inch deep and 18-inch around the top of the box. Valves shall meet AWWA C509.
12. A pre-construction meeting must be held with East Feliciana Rural Water System Personnel prior to construction.
13. Prior to construction, a DHH approval letter must be provided to the EFRWS.
14. Where fire hydrants are proposed their physical location shall be approved by the local fire district/authority. Note: As a rural system, EFRWS is not a fire rated system. Automatic flush valves are required for all dead end lines and may be required on new looped lines as well.
15. These are general specifications and other specifications may apply.

**EAST FELICIANA RURAL WATER SYSTEM**

**10270 Highway 10**

# ETHEL, LOUISIANA 70730

**(225) 683-9698 FAX (225) 683-9610**

**eastfelicianaruralwater.com**

*“This institution is an equal opportunity provider.”*

**Water Line Extension Criteria**

1. Additional lines must not have a severe adverse affect on existing system or its customers.
2. All costs associated with furnishing the service (examples - line extension and appurtenances, tapping existing system road bores, etc.) shall solely be borne by the customer or developer requesting the service.